PRODUCTION RUBRIC

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CATEGORY  | **Exceeds Standard****4 pts.** | **Meets Standard****3 pts.** | **Emerging****2 pts.** | **Attempt Made****1 pt.** | T | S |
| Single Camera Iso  | Single camera is operated correctly for the post production process.  | Single camera is operated correctly for a majority of the time, this will allow for success during the post production process. | Single camera is operated correctly for a portion of the time, this will cause challenges during the post production process. | Single camera is not operated correctly as a result the post production process is not possible.  |  |  |
| Multi Camera Iso | Multiple cameras are operated correctly for the post production process. | Multiple cameras are operated correctly for the majority of the time, this will allow for success during the post production process. | Multiple cameras are operated correctly for a portion of the time, this will cause challenges during the post production process. | Multiple cameras are not operated correctly as a result the post production process is not possible. |  |  |
| Single Camera Live | Single camera is operated correctly for the entire live production. | Single camera is operated correctly for the majority of the live production | Single camera is operated correctly for a portion of the live production. | Single camera is not operated correctly during the live production. |  |  |
| Multi Camera Live | Multiple cameras are operated correctly for the entire live production. | Multiple cameras are operated correctly for the majority of the live production | Multiple cameras are operated correctly for a portion of the live production | Multiple cameras are not operated correctly during the live production. |  |  |